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STATEMENT
The product has well capability and intact packing when leave factory. All of  the user should comply with warning item and manual, any misuse cause of the damages are not included in our guarantee, and also can not be responsible  for any malfunction & problem owing to ignore the manual.

1.Safety Instruction
Please keep this User Guide for future consultation. If you sell the unit to another user, be sure that they also receive this instruction booklet.

Unpack and check carefully there is no transportation damage before using the unit.

Before operating, ensure that the voltage and frequency of power supply  match the power requirements of the unit.

It’s important to ground the yellow/green conductor to earth in order to avoid  electric shock.

The unit must be installed in a location with adequate ventilation, at least 50cm  from adjacent surfaces. Be sure that no ventilation slots are blocked.

Disconnect main power before replacement or servicing.

Make sure there are no flammable materials close to the unit while operating as it is fire hazard.

Use safety cable when fixes this unit. DO NOT handle the unit by taking its head only, but always by taking its base.

Maximum ambient temperature is Ta: 40℃. DO NOT operate it where the temperature is higher than this Unit surface temperature may reach up to 85℃. DO NOT touch the housing bare-hand during its operation. Turn off the power and allow about 15 minutes for the unit to cool down before replacing or serving.

In the event of serious operating problem, stop using the unit immediately.Never try to repair the unit by yourself. Repairs carried out by unskilled people can lead to damage or malfunction. Please contact the nearest authorized technical assistance center. Always use the same type spare parts.

DO NOT touch any wire during operation as high voltage might be causing electric shock.

WARNING:
To prevent or reduce the risk of electrical shock or fire, do not expose the unit to rain or moisture.

DO NOT open the unit within five minutes after switching off.

The housing, the lenses, or the ultraviolet filter must be replaced if they are visibly damaged.

CAUTION:
There are no user serviceable parts inside the unit. DO NOT open the housing or attempt any repairs yourself. In the unlikely event your unit may require service, please contact your nearest dealer.

INSTALLATION:
The unit should be mounted via its screw holes on the bracket. Always ensure that the unit is  firmly fixed to avoid vibration and slipping while operating. And make sure that  the structure to which you are attaching the unit is secure and is able to support a weight of 10 times of the unit’s weight. Also always use a safety cable that can hold 12 times of the weight of the unit when installing the fixture.

The equipment must be fixed by professionals. And it must be fixed at a place where is out of the touch of people.

2.Technical Specifications
Power Voltage: AC 100-240V, 50/60Hz

Power Consumption: 150W

Light Sources: 18pcs Multi-chip 4in1 RGBW 10 Watts LED sources
Beam Angle: 25°/45°
Control 
DMX Channel: 4/8/26/72Channels
Control Modes: DMX512, Auto, Master-Slave, Music
Construction 
Display: LED Display
DMX In/Out socket: 3-pin XLR 
Power Socket: power con in/out
Protection Rating: IP20
Size
Packing Size: 1000*120*150MM
Weight
Gross Weight: 4.5Kgs
3.How to Control The Devicee

The DMX512 is widely used in intelligent lighting control,with a DMX 512 controller.connect several lights together,dmx in and dmx out, 3 pin XLR connectors: Pin 1: GND, Pin 2: Negative signal (-), Pin 3: Positive signal (+)
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XLR Pin Configuration

pinl=Ground

pin2=Data Compliment (negative)

pin3=Data true (positive)





Display:
MENU
To select the programming functions

DOWN
To go backward in the selected functions

UP
To go forward in the selected functions

ENTER
To confirm the selected functions
Set  DMX Address Code

1. Press "Menu" to "Set DMX Address",and press "ENTER" keys to enter into

2. Show "Set DMX Address DMX Address:001",Press the "UP and DOWN"

keys to amended

3 Press "ENTER" keys to save and Exit,Press the "MENU" Keys does not save and Exit
4 Functions setting via LED display panel as below:
	1
	A001
	001-512 dmx address

	2
	CH4-72
	4/8/26/72 DMX Channels

	3
	R255
	Red Color 0-255

	4
	G255
	Green Color 0-255

	5
	B255
	Blue Color 0-255

	6
	W255
	White color 0-255

	7
	FH99
	Strobe speed adjustable

	8
	WL01
	Manual choice colors

	9
	E118
	01-118 Effect choice

	10
	S220
	000-255 Effect speed adjustable

	11
	SU01
	01 strobe jump change
02 jump change


4. DMX Channel Tablee
DMX 512   4CHs 
	Channel
	Function
	Value

	CH1
	Red
	0-255

	CH2
	Green
	0-255

	CH3
	Blue
	0-255

	CH4
	White
	0-255


DMX 512   8CHs
	Channel
	Function
	Value

	CH1
	Dimmer
	Dimming from dark to bright

	CH2
	Strobe
	Strobe from slow to fast

	CH3
	Macro
	000: Dimmer mode

001-005: Choice color （CH4））

006-235: Auto run effect

236-240: Gradual change effect
241-245: Pulse change effect
246-250: Auto + Gradual + Pulse changes

251-255: Sound-Active

	CH4
	Macro speed
	Macro speed from slow to fast

	CH5
	Red
	0-255

	CH6
	Green
	0-255

	CH7
	Blue
	0-255

	CH8
	White
	0-255


DMX 512   26CHs
	Channel
	Function
	Value

	CH1
	Dimmer
	Dimming from dark to bright

	CH2
	Strobe
	Strobe from slow to fast

	CH3
	Macro
	000: Dimmer mode

001-005: Choice color （CH4））

006-235: Auto run effect

236-240: Gradual change effect
241-245: Pulse change effect
246-250: Auto + Gradual + Pulse changes

251-255: Sound-Active

	CH4
	Macro speed
	Macro speed from slow to fast

	CH5
	Red 
	0-255

	CH6
	Green 
	0-255

	CH7
	Blue 
	0-255

	CH8
	White 
	0-255

	CH9
	LED 1 
	LED Brightness, Color control with CH5-CH8

	CH10
	LED 2
	LED Brightness, Color control with CH5-CH8

	CH11
	LED 3
	LED Brightness, Color control with CH5-CH8

	CH12
	LED 4
	LED Brightness, Color control with CH5-CH8

	CH13
	LED 5 
	LED Brightness, Color control with CH5-CH8

	CH14
	LED 6
	LED Brightness, Color control with CH5-CH8

	CH15
	LED 7
	LED Brightness, Color control with CH5-CH8

	CH16
	LED 8
	LED Brightness, Color control with CH5-CH8

	CH17
	LED 9 
	LED Brightness, Color control with CH5-CH8

	CH18
	LED 10
	LED Brightness, Color control with CH5-CH8

	CH19
	LED 11
	LED Brightness, Color control with CH5-CH8

	CH20
	LED 12
	LED Brightness, Color control with CH5-CH8

	CH21
	LED 13 
	LED Brightness, Color control with CH5-CH8

	CH22
	LED 14
	LED Brightness, Color control with CH5-CH8

	CH23
	LED 15
	LED Brightness, Color control with CH5-CH8

	CH24
	LED 16
	LED Brightness, Color control with CH5-CH8

	CH25
	LED 17
	LED Brightness, Color control with CH5-CH8

	CH26
	LED 18
	LED Brightness, Color control with CH5-CH8


DMX 512   72CHs
	Channel
	Function
	Value

	CH1
	Red LED 1 
	Led dimmer from dark to bright

	CH2
	Green LED 2
	Led dimmer from dark to bright

	CH3
	Blue LED 3
	Led dimmer from dark to bright

	CH4
	White LED 4
	Led dimmer from dark to bright

	CH5
	Red LED 2
	Led dimmer from dark to bright

	CH6
	Green LED 2
	Led dimmer from dark to bright

	CH7
	Blue LED 2
	Led dimmer from dark to bright

	CH8
	White LED 2
	Led dimmer from dark to bright

	…….
	……….
	…………………………………

	…….
	……….
	…………………………………

	…….
	……….
	…………………………………

	…….
	……….
	…………………………………

	CH65
	Red LED 17
	Led dimmer from dark to bright

	CH66
	Green LED 17
	Led dimmer from dark to bright

	CH67
	Blue LED 17
	Led dimmer from dark to bright

	CH68
	White LED 17
	Led dimmer from dark to bright

	CH69
	Red LED 18
	Led dimmer from dark to bright

	CH70
	Green LED 18
	Led dimmer from dark to bright

	CH71
	Blue LED 18
	Led dimmer from dark to bright

	CH72
	White LED 18
	Led dimmer from dark to bright


5.Trouble Shooting
Following are a few common problems that may occur during operation. Here are some suggestions for easy troubleshooting:

a. The unit does not work, no light and the fan does not work

1. Check the connection of power and main fuse.

2. Measure the mains voltage on the main connector.

3. Check the power on LED.

b. Not responding to DMX controller

1. DMX LED should be on. If not, check DMX connectors, cables to see if link properly.

2. If the DMX LED is on and no response to the channel, check the address settings and DMX polarity.

3. If you have intermittent DMX signal problems, check the pins on connectors or on PCB of the unit or the previous one.

4. Try to use another DMX controller.

5. Check if the DMX cables run near or run alongside to high voltage cables that may cause damage or interference to DMX interface circuit.
6.Fixture Cleaning
The cleaning of internal and external optical lenses and/or mirrors must be carried out periodically to optimize light output. Cleaning frequency depends on the environment in which the fixture operates: damp, smoky or particularly dirty surrounding can cause greater accumulation of dirt on the unit’s optics.

· Clean with soft cloth using normal glass cleaning fluid.

· Always dry the parts carefully.

· Clean the external optics at least every 20 days. Clean the internal optics at least every 30/60 days.
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This product manual contains important information about the safe installation and use of this projector. Please read and follow these instructions carefully and keep this manual in a safe place for future reference.
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18x10W 4IN1 RGBW LED Pixel Bar Light
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